1. Install a commercially available bearing separator (A) in the gearbox housing as shown.

1. Place an appropriate size deep socket wrench (B) on the steering rack (C).

1. Set the steering gearbox in a press so the gearbox housing side points upward, then press the cylinder end seal (D) and steering rack out of the gearbox. Hold the steering rack to keep it from falling when pressed clear. Be careful not to damage the inner surface of the cylinder side on the gearbox housing with the tool.