Intermediate Shaft Installation

1. Use solvent or brake cleaner to thoroughly clean the areas where the intermediate shaft (A) contacts the transmission (differential), and dry with compressed air. Insert the intermediate shaft assembly into the differential. Hold the intermediate shaft horizontal to prevent damage to the differential oil seal (B).

1. Install the flange bolt (A) and two dowel bolts (B).

1. Install the lower torque rod.

1. Install the exhaust pipe bracket.

1. Install the right driveshaft.

1. Refill the transmission fluid.