Power Tailgate Control System - Sound Patterns of Power Tailgate Buzzer

NOTE:

- If the buzzer doesn't sound correctly, replace it.

Condition | Number of times
--- | ---
Beginning of auto open operation | 1
Beginning of auto close operation | 1
Beginning of turn over operation after pinchin | 2
Beginning of turn over operation after switch operation | 2
Vehicle speed is 5 km/h or higher during opening operation or the power tailgate system detects fall-safe | 2
Any operation is cut of time | 2
Vehicle speed is 5 km/h or higher during closing operation | 3