1. Apply Molykote M77 grease to the brake pad side of inner pad shim A, inner pad shim B both sides of outer pad shim (C), the back of pads (D), and the other areas indicated by the arrows. Wipe excess grease off the shims and brake pads. Contaminated brake discs or pads reduce stopping ability. Keep grease off the brake discs and pads.

1. Install the brake pads and pad shims correctly.Install the brake pads with the wear indicators (E) on the inside.
   If you are reusing the brake pads, always reinstall the brake pads in their original positions to prevent a momentary loss of braking efficiency.