SRS components are located in this area. Review the SRS component locations LHD , SRS Component locations RHD, and the precautions and procedures before performing repairs or service. NOTE: Check the front seat belts for damage, and replace them if necessary. Be careful not to damage them during removal and installation.
Front Seat Belt

1. Disconnect the negative cable from the battery, and wait at least 3 minutes before beginning work.

1. Slide the front seat forward fully.

1. Pull the lower anchor cover (A) back, and remove the lower anchor bolt (B).

1. Remove the center pillar lower trim, without side curtain airbags, with side curtain airbags.