MICS Function Test - Power Tailgate

1. Connect the HDS to the data link connector (DLC).

1. Select the FUNCTION TEST MENU.

   System Menu | Discription | Data List Indication
   --- | --- | ---
   Power tailgate | Power tailgate drive motor | Power tailgate motor: ON
   Power tailgate clutch | Power tailgate clutch: ON/OFF
   Power tailgate closer motor | Power tailgate closer motor: Close/Open