H/U Time Send This screen determines whether to automatically send the navigation time to the upper display. The display unit connector A (10P) passes this information to the subdisplay unit. The navigation time can be found in the Setup screen 2 ‘‘Adjust Time Zone/Clock'' setting.

- ‘‘H/U Time Send'' should always be set to ‘‘ON''.

NOTE: Selecting ‘‘Reset'' on the Adjust Time Zone/Clock screen automatically resets this diagnostic function to ‘‘ON''.