Fuse to Components Index - Under-dash Fuse/Relay Box

Under-dash Fuse/Relay Box

Fuse Number | Amps | Wire Color | Component(s) or Circuit(s) Protected
--- | --- | --- | ---
1 | 15 A | WHT/GRN | Throttle actuator control module
2 | 15 A | RED/YEL | ECM/PCM
BLK/WHT | Ignition coils
3 | 15 A | RED/WHT | Daytime running lights relay (KG model with daytime running lights)
——— | Multiplex integrated control unit
4 | 10 A | BLU/WHT | Air fuel ratio sensor
5 | 20 A | WHT/GRN | Audio unit (+ B)
6 | 10 A | WHT/BLU | Driver's door courtesy light, Front passenger's door courtesy light, Trunk light, MAP light, Driver's vanity mirror light, Passenger's vanity mirror light, Ceiling light (With sunroof), Rear individual map light
7 | 10 A | WHT | Combination switch control unit, Gauge control module, Immobilizer control unit-receiver, Immoes control unit, Navigation display unit, Navigation unit,
| Multiplex integrated control unit
8 | 20 A | ——— | Multiplex integrated control unit (+B door lock)
9 | 15 A | WHT/RED | Accessory power socket, Cigarette lighter
10 | 7.5 A | WHT | SRS unit, OPDS unit (KQ model)
11 | 30 A | GRN | Windshield wiper motor
12 | 7.5 A | RED/YEL | Multiplex integrated control unit (for rear fog light)
13 | 20 A | WHT/BLK | Front passenger's power seat recline motor
14 | 20 A | WHT/BLU | Driver's power seat slide motor
15 | 20 A | RED/BLK | Seat heater and indicator
16 | 20 A | WHT/RED | Driver's power seat recline motor
17 | 20 A | WHT/GRN | Front passenger's power seat side motor
18 | 15 A | BLK/RED | ELD unit, Secondary HO2S, Alternator, Cruise control unit, CAM sensor, Engine mount control solenoid (A/T)
19 | 15 A | BLK/YEL | ECM/PCM, Immobilizer control unit-receiver, Immoes control unit
YEL/BLK | Fuel pump
20 | 7.5 A | YEL/GRN | Windshield wiper motor, Headlight adjuster units, Headlight adjuster switch
21 | 7.5 A | YEL | Gauge control module, A/T shift lock solenoid, Back-up lights, Front passenger's power window switch indicator, Combination switch control unit, EPS control unit, Door multiplex control unit
——— | Multiplex integrated control unit
22 | 10 A | WHT/RED | SRS unit
23 | 7.5 A | ORN | ECM/PCM (LAF R)
24 | 20 A | YEL/RED | Left power window motor
25 | 20 A | YEL/BLU | Right power window motor
26 | 20 A | GRN/BLK | Front passenger's power window motor
27 | 20 A | GRN/WHT | Driver's power window motor
28 | 20 A | GRN | Sunroof motor
29 | 7.5 A | YEL/BLU | Headlight adjuster unit, Headlight adjuster switch light, Headlight adjuster control unit
30 | 7.5 A | * | Power mirror actuators, Power mirror defogger, Climate control unit (or heater control panel), Recirculation control motor, Seat heater relay
BLK/YEL | Rear window defogger relay, Blower motor relay, Radiator fan relay, condenser fan relay, A/C compressor clutch relay
31 | —— | —— | Not used
32 | 7.5 A | RED | Audio unit (ACC), Navigation display unit, Navigation unit, Accessory power socket relay ('05 KE model)
——— | Cigarette lighter relay
33 | —— | —— | Not used

*LHD type: | WHT
RHD type: | BLK/YEL