M/T Clutch Housing Countershaft Bearing Replacement

Special Tools Required Adjustable bearing puller, 45−75 mm 07YAC-0010100 Attachment, 72 x 75 mm 07746-0010600
Driver
07749-0010000
Bearing remover shaft
07JAC-PH80200
Slide hammer
07741-0010201

1. Remove the bearing set plate (A) from the clutch housing (B).

1. Remove the needle bearing (A) from the clutch houshing (B) using the special tools.

1. Install the new needle bearing (A) using the special tools.

1. Install the bearing set plate (A) with bolts (B).