1. Pull back the edge of the seat-back cover (A) all the way around, and release the clips (B), then remove the seat-back cover.

1. Install the cover in the reverse order of removal, and note these items:
   - To prevent wrinkles, make sure the material is stretched evenly over the pad before securing the clips.
   - Replace any clips you removed with new ones. Install them with commercially available upholstery ring pliers.

Left seat-back
Right seat-back