SRS Unit Replacement

Removal

1. Disconnect the battery negative cable, and wait at least 3 minutes before beginning work.

1. Disconnect both seat belt tensioner connectors.

1. Remove the center console and front panel.

1. Remove the center holder.

1. Remove the center pocket.

1. Remove the driver's and passenger's center lower cover.

1. Remove the rear vent ducts.

1. Disconnect the connectors and remove the Torx bolts (A), then pull out the SRS unit.

Installation

1. Install the new SRS unit (A) with Torx bolts (B), then connect the connectors (C) to the SRS unit; push them into position until they click.
   NOTE: Be sure the SRS unit is sitting squarely against it's bracket before torquing the Torx bolt.

1. Reconnect both seat belt tensioner connectors.

1. Reconnect the battery negative cable.

1. After installing the SRS unit, confirm proper system operation: Turn the ignition switch ON (II); the SRS indicator should come on for about 6 seconds and then go off.

1. Install all removed parts.