M/T Reverse Shift Lever Clearance Inspection

1. Measure the clearance between the reverse shift lever (A) and reverse shift fork (B) with a feeler gauge (C). If the clearance is more than the service limit, go to Step 2 .

   Standard: | 0.05−0.50 mm (0.002−0.020 in.)
   Service Limit: | 0.6 mm (0.024 in.)

1. Measure the width of the reverse shift lever.
   - If the width is not within the standard, replace the reverse shift lever.
   - If the width is within the standard, replace the reverse shift fork.

   Standard: | 6.400−6.650 mm (0.2520−0.2618 in.)

1. Measure the clearance between the reverse shift lever (A) and reverse shift piece (B) with a feeler gauge (C). If the clearance is more than the service limit, go to Step 4 .

   Standard: | 0−0.4 mm (0−0.015 in.)
   Service Limit: | 0.5 mm (0.020 in.)

1. Measure the width of the reverse shift lever.
   - If the width is not within the standard, replace the reverse shift lever.
   - If the width is within the standard, replace the reverse shift piece.

   Standard: | 13.0−13.2 mm (0.51−0.52 in.)