1. Connect the shift solenoid valve D connector with the ATF temperature sensor (F) on the shift solenoid harness.

1. Connect the solenoid valve A connector (BLU wire), solenoid valve B connector (ORN wire), solenoid valve C connector (GRN wire), and solenoid valve E connector (RED wire).

1. Install the new O-ring on the shift solenoid harness connector, and install the connector in the transmission housing.

1. Install the shift solenoid valve cover, dowel pins and a new gasket.

1. Install the new O-ring on the ATF dipstick guide pipe, and install the ATF dipstick guide pipe, then install the harness clamp on the ATF dipstick guide pipe.

1. Secure the ATF cooler line brackets on the transmission hanger with the bolts.

1. Check the connector for rust, dirt, or oil, then connect the connector securely.

1. Install the transmission lower mount nuts.

1. Install the transmission upper mount bracket, bracket plate, and ground cable, then remove the transmission jack.

1. Refill the transmission with ATF.

1. Install the battery base, then install the air cleaner housing and intake air duct.

1. Install the battery tray, battery, and battery cover, then secure the battery with its hold-down bracket. Connect the battery terminals.

1. Install the splash shield.

1. Do the power window control unit reset procedure.