DTC 11, 13, 15, 17: Wheel Sensor (Open/Short to Body Ground/Short to Power)

1. Disconnect the ABS control unit 25P connector.

1. Start the engine.

1. Measure the voltage between body ground and the appropriate wheel sensor +B and GND terminals of the ABS control unit 25P connector individually (see table).

   DTC | Appropriate Terminal
   --- | ---
   +B | GND
   11 (Right-front) | FR +B: No. 2 | FR-GND: No. 18
   13 (Left-front) | FL +B: No. 12 | FL-GND: No. 3
   15 (Right-rear) | RR +B: No. 6 | RR-GND: No. 15
   17 (Left-rear) | RL +B: No. 14 | RL-GND: No. 5

Is there 1 V or more?

YES | - | Repair short to power in the wire between the ABS modulator-control unit and the appropriate wheel sensor.■
NO | - | Go to Step 4 .

1. Turn the ignition switch OFF.