1. Install the torsion bars in the reverse order of removal, and note these items:
   - The shapes of the right torsion bar (A) and left torsion bar (B) are shown. Install the torsion bars properly.
   - Adjust the torsion bars forward or rearward with the torsion bar assembly tool.
   - Positions where each torsion bar was installed in the factory are:
     Left torsion bar: Normal position
     Right torsion bar: Higher tension
   - Make sure the trunk lid opens properly and locks securely.