CD does not eject

1. Check to see if the CD disc is ejected correctly by pushing the EJECT button.

Is it normal?

YES | - | Operation is normal.■
NO | - | Go to Step 2 .

1. Check to see if it is ejected with some binding or not ejected at all.

Is it ejected with some binding?

YES | - | Go to Step 3 .
NO | - | Go to the flow ''Power switch will not turn ON''. ■

1. Replace the disc and recheck.

Does the problem continue?

YES | - | Go to Step 4 .
NO | - | Faulty disc.■

1. Remove the audio assembly from dashboard and remove the audio unit , and check for continuity on the EJECT button using the connectors on the front printed circuit board.

Is there continuity?

YES | - | Go to Step 5 .
NO | - | Faulty front printed circuit.■

1. Remove the audio-HVAC display module unit. Check the printed circuit board and audio unit for assembling integrity.

Are they assembled correctly?

YES | - | Faulty audio unit.■
NO | - | Reinstall the printed circuit board onto the audio unit, and recheck the problem.■