SRS components are located in this area. Review the SRS component locations and the precautions and procedures, before performing repairs or service. NOTE:

- Put on gloves to protect your hands.
- Take care not to scratch the body and related parts.

1. Remove these items:
   - Front door sill trim
   - Rear door sill trim
   - Center pillar lower trim
   - Front seat belt lower anchor, both sides
   - Rear seat cushion, both sides
   - Rear seat side bolster, both sides
   - Rear seat slide linkage cover, both sides
   - Rear side trim panel, left side

1. Pull the carpet back as necessary.

1. Remove the cushion tape (A), and detach the clips (B) by using a clip remover. On RHD models, release the opener cable (C) from the clip (D).

1. Remove the fuel fill door latch (E) from the body by turning it 90 °, then remove the fuel fill door opener cable (C) from the vehicle. Take care not to kink the cable.