1. Check that the two dowel pins are installed in the clutch housing.

1. Apply urea grease UM264 (P/N 41211-PY5-305) to the release fork (A) and the release bearing (B). Install the release fork and the release bearing.

1. Place the transmission on the transmission jack, and raise it to the engine level.

1. Push the transmission towards engine until mainshaft engages with the spline of pressure plate.