Exploded View Special Tools Required Hub dis/assembly tool, 42 mm 07GAF-SD40100 Ball joint remover, 28 mm
07MAC-SL00201
or 07MAC-SL00200
Attachment, 72 x 75 mm
07746-0010600
Attachment, 78 x 90 mm
07GAD-SD40101
Driver
07749-0010000
Support base
07965-SD90100
Knuckle/Hub Replacement

1. Raise the front of the vehicle, and support it with safety stands in the proper locations.

1. Remove the wheel nuts, and front wheel.