1. Install the slider and cable assembly in the reverse order of removal, and note these items:
   - Damaged parts should be replaced.
   - Apply multipurpose grease to the glass bracket (A) and guide rail portion of the frame (B) indicated by the arrows.
   - Before reinstalling the motor, make sure both link lifters are parallel, and in the fully closed position.
   - Before reinstalling the motor, install the frame and glass, then check the opening drag.