NOTE: Review the seat replacement procedure before doing repairs or service. Removal

1. Disconnect the battery negative cable, and wait at least 3 minutes before beginning work.

1. Disconnect the appropriate side airbag 2P connector.

1. Remove the seat assembly.

1. Remove the front door sill trim and the center pillar lower trim.

1. Disconnect the floor wire harness 2P connector from the side impact sensor (first).

1. Remove the Torx bolts (A) using a Torx T30 bit, then remove the side impact sensor (first) (B).