1. If you removed the bearing outer race from the clutch housing, use the special tools to install a new bearing outer race (A) and spacer (B). There should be no space between the race, spacer, and housing.

1. With the mainshaft and countershaft removed, install the differential assembly, and bolt the transmission and clutch housing together, and tighten the bolts to 44 N·m (4.5 kgf·m, 33 lbf·ft).
   NOTE: It is not necessary to use sealing agent between the housings for this adjustment.

1. Rotate the differential assembly in both directions to seat the tapered roller bearings.