M/T Reverse Lockout Solenoid Disassembly/Reassembly

1. Write down the frequencies for the radio's preset buttons. Disconnect the negative (−) cable first, then the positive (+) cable from the battery. Remove the battery.

1. Remove the air cleaner housing.

1. Remove the battery base.

1. Carefully remove the shift cable, select cable, and cable bracket together so as not to bend the cables.

1. Disconnect the mainshaft speed sensor connector, back-up light switch connector, and reverse lockout solenoid connector.

1. Remove the bolts (A) and reverse lockout solenoid (B).

1. Remove the roller (A), the select lock return spring (C), and the select lock cam B.

1. Install in the reverse order of removal.

1. Remove the dirt and oil from the sealing surface. Apply liquid gasket (P/N 08C70-K0234M) to the sealing surface.
   NOTE: If 5 minutes have passed after applying liquid gasket, reapply it and assemble the housings. Allow it to cure at least 20 minutes after assembly before filling the transmission with oil.

1. Install the reverse lockout solenoid.

1. Connect the reverse lockout solenoid connector, back-up light switch connector, and mainshaft speed sensor connector.

1. Install the cable bracket, select cable, and shift cable.

1. Install the battery base.

1. Install the air cleaner housing.

1. Install the battery. Connect the positive (+) cable first, then the negative (−) cable to the battery.

1. Enter the anti-theft code for the radio and navigation system, then enter the customer's radio station presets.

1. Perform the power window control unit reset procedure.