1. Put the cartridge in a caulking gun, and run a bead of adhesive (A) around the edge of the quarter glass (B) as shown:
   - After applying the adhesive, peel the separator off the butyl tape.
   - Apply the adhesive within 30 minutes after applying the glass primer. Make slightly thicker bead at each corner.

1. Fold the edge of the adhesive backing from the double-sided adhesive tape stuck in Step 9 . If old quarter glass is to be reinstalled, peel the adhesive backings from the butyl tapes.