Special Tools Required P/S joint adapter (pump) 07RAK-S040111 P/S joint adapter (hose) 07RAK-S040122
P/S pressure gauge
07406-0010001
Check the fluid pressure as follows to determine whether the trouble is in the pump or gearbox.

1. Check the power steering fluid level.

1. Disconnect the pump outlet hose (A) from the pump outlet with care so as not to spill the power steering fluid on the frame and other parts. Install the P/S joint adapter (pump) on the pump outlet (B).

1. Connect the P/S joint adapter (hose) to the P/S pressure gauge, then connect the pump outlet hose to the P/S joint adapter (hose).

1. Install the P/S pressure gauge to the P/S joint adapter (pump).