Exploded View Special Tools Required Boot band tool, KD-3191 or equivalent, commercially available
Boot band pincers,
Kent-Moore J-35910
or equivalent, commercially available
NOTE: Refer to the Exploded View as needed during this procedure.
Inboard Joint Side

1. Wrap the splines with vinyl tape (A) to prevent damage to the inboard boot.

1. Install the inboard boot onto the driveshaft, then remove the vinyl tape. Be careful not to damage the inboard boot.