How to troubleshooting

1. Turn the ignition switch ON (II).

1. Connect the SCS connector (A) to the power tailgate inspection connector (B).
   - If the ignition switch is turned OFF or SCS connector is disconnected while the safe-diagonals function is working, the safe-diagnosis function stops.
   - If the power tailgate control unit does not memorize DTC, the power tailgate indicator turns on for 3 seconds, then the self-diagnosis is complete.