VSA activation indicator does not go off, and no DTCs are stored

1. Turn the ignition switch ON (II), and watch the VSA indicator.

Does the VSA indicator go off?

YES | - | Go to Step 2 .
NO | - | Do the appropriate troubleshooting for the VSA indicator.■

1. Turn the ignition switch OFF.

1. Check the VSA OFF switch.

Is the switch OK?

YES | - | Go to Step 4 .
NO | - | Replace the VSA OFF switch. ■

1. Clear the DTC using the HDS.

Does the VSA activation indicator go off?

YES | - | The system is OK at this time.■
NO | - | Go to Step 5 .

1. Do the VSA sensor neutral memorization.

1. Clear the DTC using the HDS.

Does the VSA activation indicator go off?

YES | - | The system is OK at this time.■
NO | - | Go to Step 7 .

1. Remove the gauge control module.

1. Check for continuity between the VSA OFF switch 5P connector terminal No. 2 and body ground.

Is there continuity?

YES | - | Repair short to body ground in the wire between the gauge control module and the VSA OFF switch.■
NO | - | Go to Step 9 .