1. Remove the upper radiator hose (A) and heater hoses (B).

1. Remove the engine wire harness connectors and wire harness clamps from the cylinder head.
   - Four injector connectors
   - Engine coolant temperature (ECT) sensor connector
   - Camshaft position (CMP) sensor A/B connectors
   - K20A6 engine: Exhaust gas recirculation (EGR) valve connector
   - VTEC solenoid valve connector
   - Engine oil pressure (EOP) sensor connector