1. Remove the piston from the engine block.

1. Using a ring expander (A), remove the old piston rings (B).

1. Clean all ring grooves thoroughly with a squared-off broken ring or ring groove cleaner with a blade to fit the piston grooves.
   The top and 2nd ring grooves are 1.2 mm (0.05 in.) wide. The oil ring groove is 2.0 mm (0.08 in.) wide (K20A6 engine), 2.5 mm (0.10 in.) wide (K24A3 engine).
   File down a blade if necessary.
   Do not use a wire brush to clean the ring grooves, or cut the ring grooves deeper with the cleaning tools.
   NOTE: If the piston is to be separated from the connecting rod, do not install new rings yet.