- After a collision in which the airbags or seat belt tensioners were deployed, replace the SRS unit, front sensors, and other related components. After a collision in which a side airbag was deployed, replace the side impact sensor on the deployed side and the SRS unit. After a collision in which the airbags or the side airbags did not deploy, inspect for any damage or any deformation on the SRS unit, front impact sensors, and the side impact sensors. If there is any damage, replace the SRS unit and/or the sensors.

- Do not disassemble the SRS unit, front impact sensors, or the side impact sensors.
- Turn the ignition switch OFF, disconnect the battery negative cable and wait at least 3 minutes before beginning installation or replacement of the SRS unit, or disconnecting the connectors from the SRS unit.
- Be sure the SRS unit, front impact sensors, and side impact sensors are installed securely with the mounting bolts torqued to 9.8 N·m (1.0 kgf·m, 7.2 lbf·ft)
- Do not spill water or oil on the SRS unit or the side impact sensors, and keep them away from dust.
- Store the SRS unit, front impact sensors and the side impact sensors in a cool (less than 40 °C/104 °F) and dry (less than 80 % relative humidity, no moisture) area.