DTC P2118: Throttle Actuator Current Range/Performance Problem

1. Disconnect the throttle actuator control module 16P connector.

1. Measure resistance between throttle actuator control module 16P connector terminals No. 1 and No. 8.

Is there about 1.0 Ω or less?

YES | - | Go to Step 3 .
NO | - | Substitute a known-good throttle actuator control module, then go to Step 7 and recheck. If DTC P2118 is not indicated, replace the original throttle actuator control module, then go to Step 7 .

1. Disconnect the throttle body 6P connector.