DTC P0490: EGR Control Solenoid Valve Circuit Shorted to Power

1. Turn the ignition switch ON (II).

1. Clear the DTC with the HDS.

1. Check for Temporary DTCs or DTCs with the HDS.

Is DTC P0490 indicated?

YES | - | Go to Step 4 .
NO | - | Intermittent failure, system is OK at this time. Check for poor connections or loose terminals at the EGR control solenoid valve and the ECM.■

1. Turn the ignition switch OFF.

1. Disconnect the EGR control solenoid valve 2P connector.

1. At solenoid side, measure resistance between EGR control solenoid valve 2P connector terminals No. 1 and No. 2.

Is there about 10−14 Ω at 20 °C (68 °F)?

YES | - | Go to Step 7 .
NO | - | Go to Step 11 .

1. Turn the ignition switch OFF, and wait 1 minute.

1. Disconnect ECM connector No. 1 (96P).

1. Turn the ignition switch ON (II).