ECM/PCM Inputs and Outputs at Connector D (17P)
NOTE: Standard battery voltage is 12 V.

Terminal number | Wire color | Terminal name | Description | Signal
--- | --- | --- | --- | ---
2 *2 | BRN | SMODE (SEQUENTIAL SPORT SHIFT MODE) | Detects sequential sportshift mode switch signal | In sequential sportshift mode (shift lever is positioned in sequential sportshift mode): about 0 V In other than sequential sportshift mode: about 5.0 V
3 *2 | WHT | SUP (UPSHIFT SWITCH) | Detects upshift switch signal | In sequential sportshift mode and shift lever pushed toward upshift position: about 0 V In sequential sportshift mode and shift lever in neutral position: about 5.0 V
5 *2 | GRN | ATPR (TRANSMISSION RANGE SWITCH R POSITION) | Detects transmission range switch R position signal | In R position: about 0 V In any other position: battery voltage
6 *2 | BLU | ATPP (TRANSMISSION RANGE SWITCH PARK POSITION) | Detects transmission range switch Park position signal | In Park position: about 0 V In any other position: battery voltage
8 | BRN | BKSWNC (BRAKE PEDAL POSITION SWITCH) | Detects brake pedal position switch signal | With ignition switch ON (II) and brake pedal released: battery voltage With ignition switch ON (II) and brake pedal pressed: about 0 V
9 *2 | ORN | SDN (DOWNSHIFT SWITCH) | Detects downshift switch signal | In sequential sportshift mode and shift lever pushed toward downshift position: about 0 V In sequential sportshift mode and shift lever in neutral position: about 5.0 V
9 *3 | LT BLU | CRMTCLS (CRUISE CLUTCH PEDAL POSITION SIGNAL) | Detects cruise clutch pedal position switch signal | With ignition switch ON (II) and clutch pedal released: about 0 V With ignition switch ON (II) and clutch pedal pressed: battery voltage
10 *2 | LT GRN | METINH (METER DISPLAY INHIBIT SIGNAL) | Sends inhibit signal | With ignition switch ON (II): battery voltage
15 | BRN | DBWRLY (THROTTLE ACTUATOR CONTROL MODULE RELAY) | Drives throttle actuator control module relay | With ignition switch ON (II): about 0 V

*2: | A/T
*3: | M/T