DTC P0010: VTC Oil Control Solenoid Valve Malfunction

1. Turn the ignition switch ON (II).

1. Clear the DTC with the HDS.

1. Start the engine. Hold the engine speed at 3,000 rpm (min −1 ) without load (in Park or neutral) until the radiator fan comes on, then let it idle.

1. Do the VTC TEST in the INSPECTION MENU with the HDS.

1. Check for Temporary DTCs or DTCs in the DTCs MENU with the HDS.

Is DTC P0010 indicated?

YES | - | Go to Step 6 .
NO | - | Intermittent failure, system is OK at this time. Check for poor connections or loose terminals at the VTC oil control solenoid valve and the ECM/PCM.■

1. Turn the ignition switch OFF.

1. Disconnect the VTC oil control solenoid valve 2P connector.

1. Measure resistance between VTC oil control solenoid valve 2P connector terminals No. 1 and No. 2.

Is there 6.75−8.25 Ω?

YES | - | Go to Step 9 .
NO | - | Go to Step 15 .