Master Cylinder Replacement

NOTE:

- Do not spill brake fluid on the vehicle; it may damage the paint; if brake fluid does contact the paint, wash it off immediately with water.
- The illustrations show LHD model.

1. For LHD model, remove the under-hood fuse/relay box mounting bolt (A) and the cable clamp bolt (B) from the strut bar.

1. Remove the access panel (A), then remove the driver's side strut bar (B).

1. Remove the reservoir cap and brake fluid from the master cylinder reservoir with a syringe.

1. Disconnect the brake fluid level switch connector (A).

1. Disconnect the brake lines (B) from the master cylinder (C). To prevent spills, cover the hose joints with rags or shop towels.

1. Remove the master cylinder mounting nuts (D).

1. Remove the master cylinder from the brake booster (E). Be careful not to bend or damage the brake lines when removing the master cylinder.

1. Remove the rod seal (F) from the master cylinder.
   NOTE: During installation, set the new rod seal onto the master cylinder with its grooved side (G) toward the master cylinder.

1. Install the master cylinder in the reverse order of removal, and note these items:
   - Use a new rod seal on reassembly.
   - Coat the inner boer lip and outer circumference of the new rod seal with the recommended seal grease in the master cylinder set.
   - Check the brake pedal height and free play after installing the master cylinder, and adjust it if necessary.

1. Bleed the brake system.