ABS indicator does not come on

1. Turn the ignition switch ON (II), and watch the ABS indicator.

Does the ABS indicator come on for several seconds?

YES | - | The system is OK at this time.■
NO | - | Go to Step 2 .

1. Do the gauge control module self-diagnosis function procedure.

Is gauge control module OK?

YES | - | Go to Step 3 .
NO | - | Replace gauge control module. ■

1. Turn the ignition switch OFF.

1. Remove the gauge control module.

1. Disconnect the gauge control module connector B (30P).

1. Check for continuity between gauge control module connector B (30P) terminal No. 27 and the body ground.

Is there continuity?

YES | - | Repair short to body ground in the wire between the gauge control module and the ABS modulator-control unit.■
NO | - | Check for loose treminals in the gauge control module connectors. If connectors are OK, replace the gauge control module.■