DTC P0340: CMP Sensor No Signal NOTE:

- Information marked with an asterisk ( * ) applies to the 2004 model.
- Information marked with double asterisk ( ** ) applies to the 2005 model.

1. Turn the ignition switch ON (II).

1. Clear the DTC with the HDS.

1. Start the engine. If engine does not start, keep cranking for 10 seconds.

1. Check for Temporary DTCs or DTCs with the HDS.

Is DTC P0340 indicated?

YES | - | Go to Step 5 .
NO | - | Intermittent failure, system is OK at this time. Check for poor connections or loose terminals at the CKP sensor and the ECM.■

1. Turn the ignition switch OFF.

1. Disconnect the CMP sensor 3P connector.

1. Turn the ignition switch ON (II).

1. Measure voltage between CMP sensor 3P connector terminal No. 1 and body ground.

Is there about 5 V?

YES | - | Go to Step 13 .
NO | - | Go to Step 9 .

1. Turn the ignition switch OFF, and wait 30 seconds.

1. Disconnect ECM connector No. 1 (96P).