EVAP System Troubleshooting

Special tools required Combination gauge kit 07YAJ-0010610 Tube joint adapter 07410-5790501

1. Disconnect the vacuum hose (A) from the EVAP canister (B) and connect a vacuum gauge (C) to the hose.

1. Start the engine and let it idle.
   NOTE: Engine coolant temperature must be below 65 °C (149 °F).

Is there vacuum?

YES | - | Inspect vacuum hose routing. If OK, replace the EVAP canister purge valve.■
NO | - | Go to Step 3 .

1. Hold the engine speed at 3,000 rpm (min −1 ) without load (in Park or neutral) until the radiator fan comes on, then raise the engine speed to 3,000 rpm (min −1 ).

Is there vacuum?

YES | - | Go to Step 4 .
NO | - | Inspect vacuum hose routing. If OK, replace the EVAP canister purge valve.■

1. Turn the ignition switch OFF.

1. Reconnect the vacuum hose to the EVAP canister.

1. Remove the fuel fill cap.

1. Disconnect the purge air hose (A) from the EVAP canister and connect the combination gauge kit and tube joint adapter to EVAP canister (B).

1. Remove the fuel fill cap.

1. Start the engine and raise speed to 3,000 rpm (min −1 ).

Does vacuum appear on gauge within 1 minute?

YES | - | See EVAP two way valve test to complete. Evaporative emission controls are OK.■
NO | - | Replace the EVAP canister.■