1. Check for continuity between the adaptive cruise control (ACC) unit 20P connector No. 3 terminal and body ground.

Is there continuity?

YES | - | Go to Step 27 .
NO | - | Repair an open in the wire between the adaptive cruise control (ACC) unit and the right front pressure sensor.■

1. Remove the jumper wire from the right front pressure sensor.

1. Reconnect all connectors.

1. Turn the ignition switch ON (II).