1. Install the cover in the reverse order of removal, and note these items:
   - Check the mounting holes in the back of the seat-back frame, for the clips on the seat-back top cover, for damage before reinstallation. If necessary, make them even.
   - To prevent wrinkles, make sure the material is stretched evenly over the pad before securing the clips.
   - Replace any clips (A) you removed with new ones. Install them with commercially available upholstery ring pliers (B).