DTC 44-1x (44-10 to 44-19, 44-1A to 44-1F): No Signal from the Right Side Impact Sensor (first) Special Tools Required SRS inflator simulator 07SAZ-TB4011A
SRS simulator lead H
07YAZ-S3A0100

1. Erase the DTC memory.

1. Turn the ignition switch ON (II), and check that the SRS indicator comes on for about 6 seconds and then goes off.

Does the SRS indicator stay on and is DTC 44-1x indicated?

YES | - | Go to Step 3 .
NO | - | Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures. If another DTC is indicated, go to the DTC troubleshooting index for troubleshooting details.

1. Turn the ignition switch OFF. Disconnect the battery negative cable, and wait for 3 minutes.

1. Check the connection between the floor wire harness 2P connector and the right side impact sensor (first).

Is the connection OK?

YES | - | Go to Step 5 .
NO | - | Replace the right side impact sensor (first) and/or the floor wire harness, as needed.■

1. Disconnect both seat belt tensioner 4P connectors (A).