NOTE:

- Take care not to tear the seams or damage the seat covers.
- Put on gloves to protect your hands.

1. Tilt the seat-back forward and tip the seat cushion up.

1. Remove these items:
   - Headrest and center headrest
   - Cargo net (for some models)
   - Seat-back top cover

1. Remove the bolts (A) and nut (B), disconnect the rod (C), then remove the seat-back latch (D) from the seat-back frame.

1. Install the latch in the reverse order of removal, and note these items:
   - Make sure the rod is connected securely.
   - Make sure the seat-back locks securely and unlocks properly.
   - Make sure the headrest doesn't stand still if the seat-back was unlocked.