Used engine oil may cause skin cancer if repeatedly left in contact with the skin for prolonged periods. Although this is unlikely unless you handle used oil on a daily basis, it is still advisable to thoroughly wash your hands with soap and water as soon as possible after handling used oil.

For the details of lubrication points and type of lubricants to be applied, refer to the illustrated index and various work procedures (such as Assembly/Reassembly, Replacement, Overhaul, Installation, etc.) contained in each section.

LUBRICATION POINTS | LUBRICANT
--- | ---
A | Engine | API Service Grade: SJ or SL fuel-efficient oil SAE Viscosity: See chart.
B | Manual transmission | Honda Manual Transmission Fluid (MTF) Always use genuine Honda MTF-II. Using motor oil can cause stiffer shifting because it does not contain the proper additives.
Automatic transmission | Honda ATF-Z1 Always use genuine Honda ATF-Z1. Using a non-Honda ATF can affect shift quality.
C | Brake system (including ABS line) | Brake fluid DOT 3 or DOT 4 We recommend genuine Honda Brake Fluid. Using a non-Honda brake fluid can cause corrosion and decrease the life of the system.
D | Clutch line (manual transmission) | Brake fluid DOT 3 or DOT 4
E F G | Throttle cable end (throttle link) Shift and select cable ends (manual transmission) Release fork (manual transmission) | Super High Temp Urea Grease (P/N 41211-PY5-305)
H I | Throttle cable ends Door opening detent | Silicone grease
J K L M N
O
P
Q
R
Power steering system
Brake booster clevis
Clutch master cylinder clevis
Battery terminals
Pedal linkage
Fuel fill door
Hood hinges and hood latch
Door hinges
Tailgate hinges
Multipurpose grease
S | Caliper piston boot, caliper pins, and boots | Caliper grease
T | Power steering system | Honda PSF-II Always use Honda Power Steering Fluid. Using any other type of power steering fluid or automatic transmission fluid can cause increased wear and poor steering in cold weather.
U | Air conditioning compressor | Compressor oil: KEIHIN SP-10 (P/N 38897-P13-003 or 38898-P13-003)