Special Tools Required Engine sub hanger plate 07MAK-PY30100

1. Remove all of the old liquid gasket from the oil pan mating surfaces, bolts, and bolt holes.

1. Clean and dry the oil pan mating surfaces.

1. Apply liquid gasket, P/N 08C70-K0334M or 08C70-X0331S, evenly to the engine block mating surface of the oil pan and to the inner threads of the bolt holes.
   NOTE: Do not install the parts if 4 minutes or more have elapsed since applying liquid gasket. Instead, reapply liquid gasket after removing old residue.

1. Install the oil pan.