Exploded View Removal

1. Raise the rear of the vehicle, and support it with safety stands in the proper locations.

1. Remove the rear wheel.

1. Place a floor jack under the lower arm B to support the suspension.

1. Remove the lid on the rear side trim panel.

1. Hold the damper shaft (A) with a hex wrench (B), and loosen the self-locking nut (C).

1. Remove the self-locking nut, damper mounting washer (D), and damper mounting rubber (E) from the top of damper.