1. Open the hood.

1. Disconnect the 2P connector from the hood switch.

1. Check for continuity between the terminals.
   There should be continuity between the No. 1 and No. 2 terminals when the hood is opened (lever released). There should be no continuity between the No. 1 and No. 2 terminals when the hood is closed (lever pushed down).

1. If the continuity is not as specified, replace the hood switch.