1. Reconnect the cable reel 5P (13P) connector (A) to the dashboard wire harness.
   ( ): With cruise control

1. Remove the driver's airbag assembly, and disconnect the horn switch 1P positive terminal from the cable reel (B).

1. Using a jumper wire, connect the cable reel side 1P connector (C) to body ground.
   - If the horns sound, replace the driver's airbag assembly.
   - If the horns don't sound, replace the cable reel.