Special Tools Required Wheel alignment gauge attachment 07MGK-0010100 The suspension can be adjusted for front toe and rear toe. Pre-Alignment Checks
For proper inspection and adjustment of the wheel alignment, do these checks:

1. Release the parking brake to avoid an incorrect measurement.

1. Make sure the suspension is not modified.

1. Check the tyre size and tyre pressure according to tyre information.

1. Check the runout of the wheels and tyres.

1. Check the suspension ball joints. (Hold a wheel with your hands, and move it up and down and right and left to check for wobbling.)

1. Bounce the vehicle up and down several times to stabilize the suspension.