Fuse to Components Index - Under-hood Fuse/Relay Box

Under-hood Fuse/Relay Box

Fuse Number | Amps | Wire Color | Component(s) or Circuit(s) Protected
--- | --- | --- | ---
1 | 10 A | RED/YEL | Left headlight (low beam)
2 | 30 A | ——— | Control block
3 | 10 A | WHT/YEL | Left headlight (high beam)
4 | 15 A | ——— | Control block
RED/BLK | Parking lights, Taillights, License plate lights, A/T gear position console light, Ashtray light, Audio-AVAC-display module, Cigarette lighter light, Glove box light, Hazard warning switch light, Headlight adjuster switch light, Rear individual map lights, Sunroof switch light, TCS off switch light, Radio remote switch light ('05 model), Cruise control switch light ('05 model), Navigation remote switch light ('05 model)
5 | 10 A | WHT/GRN | Right headlight (high beam)
6 | 10 A | RED/GRN | Right headlight (low beam)
7 | 7.5 A | ——— | Control block
8 | 15 A | WHT/GRN | PGM-FI main relay, Data link connector (DLC)
9 | 20 A | BLU/YEL | A/C condenser fan motor
10 | 20 A | YEL | Front fog lights (via front fog light relay), Front fog light relay
11 | 20 A | BLU/BLK | Radiator fan motor
12 | 30 A | BLU/RED | A/C compressor clutch
13 | 20 A | RED | ABS modulator-control unit, Brake lights, ECM/PCM, Horns, Ignition key light
| Ignition key light
——— | Control block
14 | 40 A | BLK/YEL | Rear window defogger, Antenna amplifier
15 | 40 A | YEL | No. 7 fuse (in the under-hood fuse/relay box), No. 5, 6, 7, 8 and 9 fuses (in the under-hood fuse/relay box)
16 | 15 A | WHT/BLK | Turn signal/hazard relay (via hazard warning switch), Hazard warning light relay
17 | 30 A | WHT/RED | ABS modulator-control unit (MR +B)
18 | 40 A (with TCS) | WHT | ABS modulator-control unit (+B FSR)
20 A (with ABS)
19 | 40 A | GRN/WHT | No. 1, 2, 3 and 4 fuses (in the under -dash fuse/relay box)
20 | 40 A | BLU | No. 12, 13, 14, 15, 16 and 17 fuses (in the under-dash fuse/relay box)
21 | 40 A | WHT/BLU | Blower motor
22 (BAT) | 100 A | ——— | Battery, Power distribution
22 (EPS) | 70 A | WHT | EPS control unit (+B)
23 (IG) | 50 A | WHT | Ignition switch, No. 12 fuse (in the under-dash fuse/relay box)
23 (P/W) | 40 A | WHT/BLU | Power window relay, No. 27, 28 fuses (in the under-dash fuse/relay box)